	--------------------------------------------
	           Mobile DT Logger Host
        	        Version 2.X
	(c) Copyright RST INSTRUMENTS LIMITED, 2017
	--------------------------------------------


1. Instructions for installing Mobile DT Logger Host software on a new Field PC
---------------------------------------------------
1.1 Using PC to FiledPC data connection

a. Install mobile device communication software (Mobile Device Center for Windows 7, 8.1 ,10).
b. Connect Field PC to the host PC using USB cable.
c. Using Windows Explorer, copy the file "RST Mobile DT Logger Host 2.XX.CAB" to a folder on Field PC ("My Documents" for example).
   2.XX represents the version number.
d. On Field PC, select Start and then File Explorer from pull down menu.
e. Navigate to the folder where the "RST Mobile DT Logger Host 2.XX.CAB" file was copied to.
f. Click on "RST Mobile DT Logger Host 2.XX.CAB" file and follow installation instructions.

1.2 Using USB flash memory on new FieldPC2

a. Using Windows Explorer, copy the file "RST Mobile DT Logger Host 2.XX.CAB" to a USB flash memory.
b. Eject USB flash memory from PC and insert into FieldPC2 USB port 
c. On Field PC, select Start and then File Explorer from pull down menu.
d. Navigate to flash drive location, named “Hard drive”.
e. Click on "RST Mobile DT Logger Host 2.XX.CAB" file and follow installation instructions.

2. Setting Start Menu - old Field PC only
--------------------------------------------------
The following procedure will modify the start menu so the Mobile DT Logger Host Host
shortcut icon will be displayed. Note, this is required since a maximum of 9
items can be displayed in the start menu.

a. Click Start and then Settings
b. Click "Menu" icon
c. Uncheck Inbox, or any other item that will not be required.
d. Check Mobile DT Logger Host
e. Click "Ok" button

3. Installing USB drivers.
------------------------------------------------------------------
The USB driver files are installed during Mobile DT Logger Host software installation,
but MS Windows Mobile might ask for the file name when used for the first time.

a. After Mobile DT Logger Host software is successfully installed, plug the USB cable "A" plug into readout unit.
b. If prompted for a driver name - use "ftdi_ser.dll" in full.

4. Instructions for uninstalling Mobile DT Logger Host software from Field PC
------------------------------------------------------------------
a. Click Start, then Settings,System,Remove Programs
b. Select "RST Mobile DT Logger Host 2.XX"
c. Click "Remove" button


------------------------------------------------------------------

